**Configure IP Addresses and DHCP**

enable

configure terminal

interface gigabitethernet0/0

ip address 192.168.1.1 255.255.255.0

no shutdown

exit

ip dhcp pool LAB\_NETWORK

network 192.168.1.0 255.255.255.0

default-router 192.168.1.1

exit

**Practice Troubleshooting Scenarios**

configure terminal

no ip dhcp pool LAB\_NETWORK